|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| serial number | name | Production t/a | Solid waste classification | Utilization and Disposal Measures |
| 1 | Impurities filtered by the rubber filter | 1.35 | generally  solid waste | Environmental sanitation department unified disposal |
| 2 | Steel wire trim | 10.0 | Comprehensive utilization of external sales |
| 3 | Hose scraps | 3.4 | Comprehensive utilization of external sales |
| 4 | waste packaging material | 1.0 | Comprehensive utilization of external sales |
| 5 | Household garbage | 15.9 | Environmental sanitation department unified disposal |
| 6 | Bag dust collector dust | 0.828 | In-plant recycling |
| 7 | Old water bag cloth and waste plastic cloth | 8.2 | Comprehensive utilization of external sales |
|  | unqualified product | 10.3 | Comprehensive utilization of external sales |
| 8 | waste engine oil | 0.2 | Hazardous waste HW08 | Regularly sent to Xingtai Jiatai Environmental Protection Technology Co., Ltd. for proper disposal |
| 9 | waste activated carbon | 1.2 | Hazardous waste HW49 |
| 10 | water treatment sludge | 0.3 | Hazardous waste HW49 |
| 11 | total | 52.678 | Comprehensive utilization or proper disposal | |

Handan Snoop Rubber Hose Co., Ltd.

Publicity Form of Solid Waste Generation and Disposal

Waste activated carbon, waste engine oil, and water treatment sludge are hazardous waste. Special storage devices are set up and sent to the hazardous waste storage room for temporary storage. They are regularly sent to qualified hazardous waste disposal units for proper disposal . Hazardous waste storage rooms should be constructed in accordance with the requirements of the Hazardous Waste Storage Pollution Control Standard (GB18597-2001); at the same time, hazardous waste warning signs should be set up, managed by special personnel, and records of hazardous waste discharge and disposal should be kept. At the same time, hazardous solid waste is not stored in the factory for a long time, and the waste is transported in a closed manner during transportation to avoid harm to the environment along the way.

After taking the above measures, the solid waste produced by the project has been properly disposed of, and the solid waste will not be discharged outside during the operation period, which has little impact on the surrounding environment .